---
summary: "Android app (node): connection runbook + Connect/Chat/Voice/Canvas command surface"
read_when:
  - Pairing or reconnecting the Android node
  - Debugging Android gateway discovery or auth
  - Verifying chat history parity across clients
title: "Android App"
---

# Android App (Node)

## Support snapshot

- Role: companion node app (Android does not host the Gateway).
- Gateway required: yes (run it on macOS, Linux, or Windows via WSL2).
- Install: [Getting Started](/start/getting-started) + [Pairing](/channels/pairing).
- Gateway: [Runbook](/gateway) + [Configuration](/gateway/configuration).
  - Protocols: [Gateway protocol](/gateway/protocol) (nodes + control plane).

## System control

System control (launchd/systemd) lives on the Gateway host. See [Gateway](/gateway).

## Connection Runbook

Android node app ⇄ (mDNS/NSD + WebSocket) ⇄ **Gateway**

Android connects directly to the Gateway WebSocket (default `ws://<host>:18789`) and uses device pairing (`role: node`).

### Prerequisites

- You can run the Gateway on the “master” machine.
- Android device/emulator can reach the gateway WebSocket:
  - Same LAN with mDNS/NSD, **or**
  - Same Tailscale tailnet using Wide-Area Bonjour / unicast DNS-SD (see below), **or**
  - Manual gateway host/port (fallback)
- You can run the CLI (`openclaw`) on the gateway machine (or via SSH).

### 1) Start the Gateway

```bash
openclaw gateway --port 18789 --verbose
```

Confirm in logs you see something like:

- `listening on ws://0.0.0.0:18789`

For tailnet-only setups (recommended for Vienna ⇄ London), bind the gateway to the tailnet IP:

- Set `gateway.bind: "tailnet"` in `~/.openclaw/openclaw.json` on the gateway host.
- Restart the Gateway / macOS menubar app.

### 2) Verify discovery (optional)

From the gateway machine:

```bash
dns-sd -B _openclaw-gw._tcp local.
```

More debugging notes: [Bonjour](/gateway/bonjour).

#### Tailnet (Vienna ⇄ London) discovery via unicast DNS-SD

Android NSD/mDNS discovery won’t cross networks. If your Android node and the gateway are on different networks but connected via Tailscale, use Wide-Area Bonjour / unicast DNS-SD instead:

1. Set up a DNS-SD zone (example `openclaw.internal.`) on the gateway host and publish `_openclaw-gw._tcp` records.
2. Configure Tailscale split DNS for your chosen domain pointing at that DNS server.

Details and example CoreDNS config: [Bonjour](/gateway/bonjour).

### 3) Connect from Android

In the Android app:

- The app keeps its gateway connection alive via a **foreground service** (persistent notification).
- Open the **Connect** tab.
- Use **Setup Code** or **Manual** mode.
- If discovery is blocked, use manual host/port (and TLS/token/password when required) in **Advanced controls**.

After the first successful pairing, Android auto-reconnects on launch:

- Manual endpoint (if enabled), otherwise
- The last discovered gateway (best-effort).

### 4) Approve pairing (CLI)

On the gateway machine:

```bash
openclaw devices list
openclaw devices approve <requestId>
openclaw devices reject <requestId>
```

Pairing details: [Pairing](/channels/pairing).

### 5) Verify the node is connected

- Via nodes status:

  ```bash
  openclaw nodes status
  ```

- Via Gateway:

  ```bash
  openclaw gateway call node.list --params "{}"
  ```

### 6) Chat + history

The Android Chat tab supports session selection (default `main`, plus other existing sessions):

- History: `chat.history`
- Send: `chat.send`
- Push updates (best-effort): `chat.subscribe` → `event:"chat"`

### 7) Canvas + camera

#### Gateway Canvas Host (recommended for web content)

If you want the node to show real HTML/CSS/JS that the agent can edit on disk, point the node at the Gateway canvas host.

Note: nodes load canvas from the Gateway HTTP server (same port as `gateway.port`, default `18789`).

1. Create `~/.openclaw/workspace/canvas/index.html` on the gateway host.

2. Navigate the node to it (LAN):

```bash
openclaw nodes invoke --node "<Android Node>" --command canvas.navigate --params '{"url":"http://<gateway-hostname>.local:18789/__openclaw__/canvas/"}'
```

Tailnet (optional): if both devices are on Tailscale, use a MagicDNS name or tailnet IP instead of `.local`, e.g. `http://<gateway-magicdns>:18789/__openclaw__/canvas/`.

This server injects a live-reload client into HTML and reloads on file changes.
The A2UI host lives at `http://<gateway-host>:18789/__openclaw__/a2ui/`.

Canvas commands (foreground only):

- `canvas.eval`, `canvas.snapshot`, `canvas.navigate` (use `{"url":""}` or `{"url":"/"}` to return to the default scaffold). `canvas.snapshot` returns `{ format, base64 }` (default `format="jpeg"`).
- A2UI: `canvas.a2ui.push`, `canvas.a2ui.reset` (`canvas.a2ui.pushJSONL` legacy alias)

Camera commands (foreground only; permission-gated):

- `camera.snap` (jpg)
- `camera.clip` (mp4)

See [Camera node](/nodes/camera) for parameters and CLI helpers.

### 8) Voice + expanded Android command surface

- Voice: Android uses a single mic on/off flow in the Voice tab with transcript capture and TTS playback (ElevenLabs when configured, system TTS fallback). Voice stops when the app leaves the foreground.
- Voice wake/talk-mode toggles are currently removed from Android UX/runtime.
- Additional Android command families (availability depends on device + permissions):
  - `device.status`, `device.info`, `device.permissions`, `device.health`
  - `notifications.list`, `notifications.actions`
  - `photos.latest`
  - `contacts.search`, `contacts.add`
  - `calendar.events`, `calendar.add`
  - `motion.activity`, `motion.pedometer`
